**Assembly Notes**

1. Make sure to connect 12V power via 2.5mm DC Power Jack.

2. Voltage Regulator should be horizontal mounted and equipped with a heatsink.

3. C1 must be an electrolytic capacitor.